# open Coap related issues on Gitlab

|  |  |  |  |
| --- | --- | --- | --- |
| **Device** | **Issue** | **Description** | **Remarks** |
| *Device independent* | <https://gitlab.allterco.net/Dimitrov/shellyqa-group/issues/83> | [openhab] FTR Status update of settings update |  |
| Plug-S | <https://gitlab.allterco.net/Dimitrov/shellyqa-group/issues/93> | Shelly Plug-S: Coap description incorrect |  |
| Plug-S | <https://gitlab.allterco.net/Dimitrov/shellyqa-group/issues/94> | Shelly Plug-S: Coap/REST power meter values data type not consistent |  |
| RGBW2 | <https://gitlab.allterco.net/Dimitrov/shellyqa-group/issues/95> | Shelly RGBW2: Coap description VSwitch |  |
| RGBW2 | <https://gitlab.allterco.net/Dimitrov/shellyqa-group/issues/96> | Shelly RGBW2: Missing power meter values in Coap payload | Added in 1.6rc4 |
| 1PM | <https://gitlab.allterco.net/Dimitrov/shellyqa-group/issues/97> | Shelly 1PM: Coap description incorrect |  |
| 1PM | <https://gitlab.allterco.net/Dimitrov/shellyqa-group/issues/98> | Shelly 1PM: Coap/REST power meter values data type not consistent |  |
| 2.5 relay mode | <https://gitlab.allterco.net/Dimitrov/shellyqa-group/issues/99> | Shelly 2.5 Relay Mode: Coap description incorrect |  |
| 2.5 relay mode | <https://gitlab.allterco.net/Dimitrov/shellyqa-group/issues/100> | Shelly 2.5 Relay Mode: Coap/REST power meter values data type not consistent |  |
| 2.5 roller mode | <https://gitlab.allterco.net/Dimitrov/shellyqa-group/issues/101> | Shelly 2.5 Roller Mode: Coap description incorrect |  |
| 2.5 roller mode | <https://gitlab.allterco.net/Dimitrov/shellyqa-group/issues/102> | Shelly 2.5 Roller Mode: Coap/REST power meter values data type not consistent |  |
| Dimmer | <https://gitlab.allterco.net/Dimitrov/shellyqa-group/issues/103> | Shelly Dimmer: Coap description not consistent |  |
| Dimmer | <https://gitlab.allterco.net/Dimitrov/shellyqa-group/issues/104> | Shelly Dimmer: Coap/REST power meter values data type not consistent |  |
| Duo | <https://gitlab.allterco.net/Dimitrov/shellyqa-group/issues/105> | Shelly DUO: Coap/REST power meter values data type not consistent |  |
| Duo | <https://gitlab.allterco.net/Dimitrov/shellyqa-group/issues/107> | Inconsistent Coap descriptions with Duo |  |